To update the DIGIPAD8 firmware you need to use the PROEL UPDATE TOOL application. The firmware update to be installed is downloaded from the web so you need to have an active internet connection.
Please, follow the instructions below.

1) Install the PROEL UPDATE TOOL application on your Windows PC.
2) Launch the PROEL UPDATE TOOL application and press OK to select DIGIPAD8.
3) In the next windows you can see which is the latest firmware version available (firmware_VX.X.X.XX.XX.bin): check in the SYSTEM page of the DIGIPAD8 menu which is the current firwmare version installed and if you need to update.
4) If you want to proceed with the update, press DOWNLOAD button: the firmware file is then downloaded to your computer. Once the download is complete, press the GO TO UPDATE button.
5) The firmware update occurs in two phases: the first phase for the UI (user interface) and the second phase for the DSP. For each phase you will find a HELP button on the page: press the relevant button and follow the instructions on the screen.
6) Please do UI update first and then DSP update.
7) Once the update has been completed you will need to perform a RESTORE FACTORY in the SYSTEM page of the DIGIPAD8 menu.


DIGIPAD8 Firmware Release V1.3.0.12.21
April 2026
What’s new:
- Introduction of the EQ graphic interface in the touch screen display.
- Improved mixer response to app commands.
- Elimination of mute when loading a scene.
- Simplified firmware update procedure.
- Optimization of stereo channels 5/6 and 7/8.


PROEL S.p.A.
2026